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	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN 
	SN:
	Nº da OS      
	TLN:02623

	                      6821322
	                         12867                                         
	039482
	

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	QUANT:

	           TU. MÉXICO: 750585
	                         REAR BEARING SUPPORT
	1

	
	
	
	

	ITEM
(Item)
	DESCRIÇÃO DO SERVIÇO A EXECUTAR
 (Description of the work to be executed)
	EXECUÇÃO
(Execution)
	*SETOR/FORNECEDOR
(Sector/Supplier)

	1
	EXECUTAR FPI: ASTM E 1417, METHOD-A, LEVEL 3.
APRESENTOU INDICAÇÃO? (  )SIM             (  )NÃO

RUN FPI: ASTM E 1417, METHOD-A, LEVEL 3. DID YOU PRESENT AN INDICATION? ( )YES ( )N
	
	NDT

	2
	LIMPAR, SEM DESMARCAR. IP-0006, 3.10

CLEAN, WITHOUT DESELECTING. IP-0006, 3.1
	
	LIMPEZA

	3
	INSPEÇÃO: ANALISAR E REPROGRAMAR PARA REFORÇAR OS 4- KEY SLOTS E FECHAR OS FUROS DO HAT BAND, MENOS 1. AMS 5674347SS)
END e USINAR AS FACES E DIÂMETROS.
GLASS BEAD E LIMPEZA.

INSPECTION: ANALYZE AND REPROGRAM TO REINFORCE THE 4- KEY SLOTS AND CLOSE THE HAT BAND HOLES, MINUS 1. AMS 5674347SS) END AND MACHINE THE FACES AND DIAMETERS. GLASS BEAD AND CLEANING
	
	INSPEÇÃO

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):   VILSON BARBOSA
	DATA 
(Date):   26/11/2024

	[bookmark: Texto2]     
	VILSON BARBOSA
	26/11/2024


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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