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	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:

	23005655
	CAG-95742
	--
	2118

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	CAG – 95742 (M250 C30P)
	RGB ASSY
	DESMONTAGEM / DISASSEMBLY	1

	TSN:
	CSN:
	TSO:
	CSO:

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	
	M250	DESMONTAGEM / DISASSEMBLY	Realizar desmontagem do módulo de gearbox.

NOTA: SE DURANTE A DESMONTAGEM FOR DETECTADO ALGUMA ANORMALIDADE REALIZAR O REGISTRO FOTOGRÁFICO.

Disassemble the gearbox module.

NOTE: IF ANY ABNORMALITY IS DETECTED DURING DISASSEMBLY, TAKE A PHOTOGRAPHIC RECORD.

	
	CHEMICAL CLEANING	LIMPAR / CLEAN	Realizar limpeza do módulo de gearbox utilizando como referência o OHM – 10W3 e o formulário FS.957.

Perform cleaning of the gearbox module per OHM –10W3 and the form FS.957 as a reference.

	
	CHEMICAL CLEANING	NON-DESTRUCTIVE TESTING	Realizar NDT do módulo de gearbox como referência o OHM – 10W3 e o formulário FS.957.

Perform NDT of the gearbox module per OHM – 10W3 and the form FS.957 as a reference.

	
	CHEMICAL CLEANING	LIMPAR / CLEAN	Realizar limpeza pós-NDT do módulo de gearbox utilizando como referência o OHM – 10W3 e o formulário FS.957.

Perform cleaning post NDT of the gearbox module per OHM – 10W3 and the form FS.957 as a reference.

	
	CHEMICAL CLEANING	PRESERVAÇÃO / PRESERVATION	Realizar preservação dos eixos, engrenagens, rolamentos e artigos propensos a corrosão conforme OHM – 10W3.

Perform preservation of shafts, gears, bearings, and any parts that can get corroded without oil preservation per OHM – 10W3.

	
	M250	INSPEÇÃO / INSPECTION	Realizar inspeção do módulo de gearbox utilizando como referência o
OHM - 10W3 efetuando os registros nos formulários FS.0942.

NOTA: SOLICITAR O.S. FILHA ESPECÍFICA DE CADA COMPONENTE CONFORME
NECESSÁRIO.

Perform inspection of the gearbox module per OHM - 10W3 as a
reference, making the records on forms FS.0942.

NOTE: REQUEST SUB W. O. OF EACH COMPONENT AS NEEDED.

	
	M250	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.

Final inspection.

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
(Date):

	
	Daniel Hoskem
	12/12/24


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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