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Descrição gerada automaticamente]
	REGISTRO
	REVISÃO
	1

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN(PN):
	SN:
	ARTIGO/PARTE(Article/Part):
	QUANT:
	TLN:
	Nº da OS(WO):

	393291-21
	LMG3269-16
	QEC ASSY
	1
	T.O 1C-130A-36
	040128

	ITEM
(Item)
	DESCRIÇÃO DO SERVIÇO A EXECUTAR
(Description of thework to be executed)
	EXECUÇÃO
(Execution)
	*SETOR/FORNECEDOR
(Sector/Supplier)

	
	
EXECUTAR LIMPEZA E DECAPAGEM DE TODAS AS PARTES DO Q.E.C CONFORME IP006, ITENS 3.35 E 3.18

PERFORM CLEANING AND STRIPPING OF ALL PARTS OF THE Q.E.C. IN ACCORDANCE WITH IP006, ITEMS 3.35 AND 3.18

	
	
LIMPEZA

	
	REALIZAR EDDY CURRENT INSPECTION NAS SEGUINTES AREAS ABAIXO CONFORME T.O 1C-130A-36 (ANEXA):

PERFORM EDDY CURRENT INSPECTION IN THE FOLLOWING AREAS BELOW IN ACCORDANCE WITH T.O 1C-130A-36 (ATTACHED):


6-11. – INSPECTION N-2 (AREAS A, B E C) : QEC LONGERONS, FIREWALL FRAME FORGING AND FIREWALL ASSEMBLY (FIGURA 6-2)

6-27A. – INSPECTION N-5 (GEARBOX ALIGNMENT HOLE) : QEC LOWER LONGERON RADIUS AREAS (FIGURA 6-3)

6-28. – INSPECTION N-6 (AREAS A, B, C e D) : AFT ENGINE MOUNT BEAM AND AFT ENGINE MOUNT BEAM SUPPORTS (FIGURA 6-4, SHEET 1 E 2)


FORAM ENCONTRADAS INDICAÇÕES?
INDICATIONS WERE FOUND

(     ) SIM – VER IAS RG-0332 ANEXO
         YES – SEE IAS RG-0332 ANNEX

(     ) NÃO
         NO


OBS: FAZER LAUDO SEPARADO PARA CADA AREA INSPECIONADA.
NOTE: MAKE A SEPARATE REPORT FOR EACH INSPECTED AREA.

	
	NDT IAS

	
	REALIZAR LIMPEZA PÓS NDI CONFORME IP-006, ITEM 3.34.
PERFORM POST-NDI CLEANING IN ACCORDANCE WITH IP-006, ITEM 3.34.

	
	LIMPEZA

	1
	REALIZAR INSPEÇÃO APÓS OPERAÇÃO DE NDI.
PERFORM INSPECTION AFTER NDI OPERATION

REFIRA-SE AOS RESULTADOS REGISTRADOS NO IAS RG-0332 (CASO TENHA) E PREENCHER O MESMO COM DEVIDAS OBSERVAÇÕES.
REFER TO THE RESULTS RECORDED IN IAS RG-0332 (IF ANY) AND FILL IT OUT WITH APPROPRIATE OBSERVATIONS.



AVALIAR OS LIMITES SE ACEITAÇÃO CONFORME MANUAL T.O 1C-130A-36
EVALUATE ACCEPTANCE LIMITS IN ACCORDANCE WITH MANUAL T.O 1C-130A-36


(     ) APROVADO / APPROVED
         
(     ) REJEITADO / REJECTED


AREA N-2 - ANEXAR N° LAUDO NDI:________________
                   ATTACH NDI REPORT NO.

AREA N-5 - ANEXAR N° LAUDO NDI:________________
                     ATTACH NDI REPORT NO.

AREA N-6 - ANEXAR N° LAUDO NDI:________________
                     ATTACH NDI REPORT NO.

	
	INSPEÇÃO

	3
	INSPEÇÃO FINAL

FINAL INSPECTION.

	
	INSPEÇÃO

	
	
	
	

	
	
	
	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA
(Date):

	T.O. 1C-130A-36 - SECTION VI 
NACELLE GROUP
NONDESTRUCTIVE INSPECTION (NDI) OF NACELLE.
6-11. – INSPECTION N-2
6-27A. – INSPECTION N-5
6-28. – INSPECTION N-6

	Leonardo S Gomes
	
13/01/2025



· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
	




image3.wmf
Int.


image4.wmf
Ext.


image1.wmf
Int.


image2.wmf
Ext.


image5.png




