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	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
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	QUANT:
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	RRE-200839
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	DESCRIÇÃO
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	ACESSÓRIOS	DESMONTAGEM / DISASSEMBLY	DISASSEMBLY PTG
IAW CMM WITH IPL ATA 73-20-16
DISASSEMBLY:

Perform Initial Disassembly Procedures. Refer to item 3
Dissasemble of Cover Assembly. Refer to item 4.
Disassembly of Drive Body Assembly. Refer to item 5.

Faça os procedimentos iniciais de desmontagem. Refira-se ao item 3.
Desmonte o Cover Assembly. Refira-se ao item 4.
Desmonte o Drive Body Assembly. Refira-se ao item 5.


	
	ACESSÓRIOS	LIMPAR / CLEAN	CLEAN PTG
IAW CMM WITH IPL ATA 73-20-16,
CLEANING:

Exterior Cleaning Procedures. Refer to item 2
Cleaning Metallic Parts, Refer to item 3.
Remove Corrosion from Aluminum Parts. Refer to item 4.
Remove Rust from Steel Parts. Refer to item 5.
Clean Close-Fitting Parts and Matched Assemblies. Refer to item 6.
Clean Filters and Restrictors. Refer to item 7.
Specific Cleaning Instructions, Refer to item 8.


Procedimento de limpeza externa, Refira-se ao item 2
Limpe as partes metálicas. Refira-se ao item 3.
Remova a corrosão das peças de alumínio. Refira-se ao item 4.
Remova a ferrugem das peças de aço. Refira-se ao item 5.
Limpe as partes Close-Fitting e os Matched Assemblies. Refira-se ao item 6.
Limpe os filtros e restritores. Refira-se ao item 7.
Instruções de limpeza especifica, Refira-se ao item 8.



	
	ACESSÓRIOS	INSPEÇÃO / INSPECTION	CHECK PTG
IAW CMM WITH IPL ATA 73-20-16,
CHECK:

Perform General Checks. Refer to item 3.
Perform check of Power Turbine Governors Involved in Fires,  Refer to item 4.
Perform Fluorescent Penetrant Inspection, Refer to item 5.
Perform Magnetic Particle Inspection. Refer to item 6.
Perform Demagnetization of Steel Parts. Refer to item 7.
Follow Specific Check Procedures, Rerfer to item 8.
Perform Union Filter Assembly Load Test, Refer to item 9.


Faça os cheques gerais. Refira-se ao item 3.
Faça a checagem do Power Turbine Governors Involved in Fires, Refira-se ao item 4.
Faça a inspeção com Penetrante Fluorescente, Refira-se ao item 5.
Faça a inspeção por partículas magnéticas. Refira-se ao item 6.
Faça a desmagnetização das partes de aço. Refira-se ao item 7.
Siga os Procedimentos de Verificação Específicas, Refira-se ao item 8.
Realizar o Union Filter Assembly Load Test, Consulte o item 9.


	
	ACESSÓRIOS	REPARAR - ACESSORIOS / REPAIR - ACCESSORIES	REPAIR PTG
IAW CMM WITH IPL ATA 73-20-16, REPAIR:

If necessary, repair Nicks, Scratches, and Burrs. Refer to item 4.
If necessary, repair Identification Plate Screw Hole. Refer to item 5.
If necessary, repair Dry Film Lubricant, Refer to item 6.
If necessary, repair Governor Lever Assembly, Refer to item 7.
If necessary, repair overspeed Lever Assembly, Refer to item 8.
If necesary, replace Drive Shaft Teflon Tube, Refer to item 9.
If necessary, repair Drive Shaft Pin Hole, Refer to item 10.
If necessary, repair Bearing Retainer, Refer to item 11.
If necessary, Repair  Drive Body PG and PY Ports, Refer to item 12.
If necesary make Drive Body Rework Procedure, Refer to item 13.
If necessary, repair Drive Body Set Screw Hole , Refer to item 14.
If necessary, replace Cover Assembly Valve Seat , Refer to item 15.
If necessary, replace Cover Assembly Throttle Shaft Bushing, Refer to item 16.
If necessary, Repair of Lock Patch, Refer to item 17.
If necessary, repair Bearing Cap, Refer to item 18.
If necessary, repair Bushing Assembly, Refer to item 19.
If necessary, repair Throttle Shaft, Refer to item 20.
If necessary, repair Throttle Cam, Refer to item 21.
If necessary,  Rebraze of Loose Pointer in Stop Lever Assembly, Refer to item 22.

Se necessário, repare nicks, arranhões e rebarbas. Refira-se ao item 4.
Se necessário, repare o furo da placa de identificação. Refira-se ao item 5.
Se necessário, repare o Dry Film Lubricant, Refira-se ao item 6.
Se necessário, repare o  Governor Lever Assembly, Refira-se ao item 7.
Se necessário, repare o overspeed Lever Assembly, Refira-se 8.
Se necessário, substitua o Drive Shaft Teflon Tube, Refira-se ao item 9.
Se necessário, repare o Drive Shaft Pin Hole, Refira-se ao item 10.
Se necessário, repare o Bearing Retainer, Refira-se ao item 11.
Se necessário, repare o  Drive Body PG and PY Ports, Refira-se ao item 12.
Se necessário, faça o procedimento de retrabalho do Drive Body, Refira-se ao item 13.
Se necessário, repare o Drive Body Set Screw Hole, Refira-se ao item 14.
Se necessário, substitua o Cover Assembly Valve Seat, Refira-se ao item 15.
Se necessário, substituia o Cover Assembly Throttle Shaft Bushing, Refira-se ao item 16.
Se necessário, substitua o  Lock Patch, Refira-se ao item 17.
Se necessário, repare o Bearing Cap, Refira-se ao item 18. Se necessário, repare o Bushing Assembly, Refira-se ao item 19.
Se necessário, repare o Throttle Shaft, Refira-se ao item 20.
Se necessário, repair o Throttle Cam, Refira-se ao item 21.
Se necessário, faça o rebrazamento do Loose Pointer in Stop Lever Assembly, Refira-se ao item 22.


	
	ACESSÓRIOS	MONTAG EM/ ASSEMBLY	ASSEMBLY PTG
IAW CMM WITH IPL ATA 73-20-16, ASSEMBLY:

If applicable, Perform Installation of Threaded Fasteners, Refer to item 3.
Perform the necessary service according to steps 4 to 8 in according with manual.
Assembly governor and Overspeed Levers , Refer to item 9.
Perform the installation of PG and PY Restrictors, Refer to item 10.
Perform the Assembly and installation of Drive Shaft, Refer to item 11.
Assembly of Cover Assembly, Refer to item 12.
Assembly of Drive Body and Cover Assembly, Refer to item 13.
Perform the Final Assembl, Refer to item 14

Se aplicável, Realize a instalação  do Threaded Fasteners, Refira-se ao item 3.
Realizar o serviço necessário de acordo com as etapas 4 até 8 de acordo com manual
Monte o governor and Overspeed Levers, Refira-se ao item 9
Realize a instalação do PG and PY Restrictors, Refira-se ao item 10.
Realize a montagem e a instalação do Drive Shaft, Refira-se ao item 11.
Monte o Cover Assembly, Refira-se ao item 12.
Monte o Drive Body and Cover Assembly, Refira-se ao item 13.
Realize a montagem final, Refira-se ao item 14.

	
	ACESSÓRIOS	TESTE /TEST	TEST PTG IAW CMM WITH IPL ATA 73-20-16, TESTING:

Perform the Final Bleed Block Simulator Calibration, Refer to item 3.
Perform the test connections, Refer to item 4.
Run-as-Received Testing. Refer to item 8;
Perform Final Calibration. Refer to item 9.

Realize a calibração do simulador de bloco de sangria, Refira-se ao tem 3.
Realize o teste de conexões, Refira-se ao item 4.
Faça o teste as-received. Refira-se ao item 8;
Faça a calibração final. Refira-se ao item 9.

	
	ACESSÓRIOS	APROVAÇÃO FINAL DO SERVLÇO REALIZADO / FINAL APPROVAL OF THE SERVICE	INSPEÇÃO FINAL
FINAL INSPECTION
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	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
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· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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