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	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	2
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-A, LEVEL-3.
PRESTAR ESPECIAL ATENÇÃO NAS ÁREAS DE ESTRESSES, CONFORME MOSTRA A FIGURA ANEXA.
APRESENTOU INDICAÇÃO?   (  )SIM      (  )NÃO

RUN FPI: ASTM E 1417, METHOD-A, LEVEL-3. PAY SPECIAL ATTENTION TO AREAS OF STRESS, AS SHOWN IN THE ATTACHED FIGURE. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	3
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	4
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	PASSAR ALARGADOR NOS 2- FUROS ONDE PASSAM OS EYE BOLTS.  VEJA A FIGURA ANEXA.

PASSAR UMA BROCA DE 0.312¨ NOS FUROS DA FACE MAIOR, ADJACENTES AOS STUDS DE UNIÃO.

APPLY REAMER IN THE 2- HOLES WHERE THE EYE BOLTS PASS. SEE THE ATTACHED FIGURE. PASS A 0.312 ° DRILL BIT INTO THE HOLES ON THE LARGER FACE, ADJACENT TO THE JOINING STUDS.

	5
	REPAIR SHOP	ISOLAÇÃO / MASK	ISOLAR OS STUDS, INSERTS, FUROS E ÁREAS DE CONTATO.

ISOLATE STUDS, INSERTS, HOLES AND CONTACT AREAS.

	6
	REPAIR SHOP	PINTURA / PAINTING	PINTAR EXTERNAMENTE:
PRIMER PA-0060
CINZA PA-0065

PAINTING EXTERNALLY: FIRST PA-0060 CINZA PA-0065

	7
	REPAIR SHOP	REMOVER ISOLAMENTO / REMOVE MASK	REMOVER AS ISOLAÇÕES E OS EXCESSOS DE TINTA.

REMOVE INSULATION AND EXCESS PAINT.

	8
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	LIMPAR AS ROSCAS DOS STUDS E INSERTS.

CLEAN THE THREADS OF THE STUDS AND INSERTS.

	9
	CHEMICAL CLEANING	INSPEÇÃO / INSPECTION	LIMPAR COM PRESSÃO TODAS AS ENTRANÇAS E VIAS. IP-0006, 3.9

PRESSURE CLEAN ALL BRAIDS AND TRACKS. IP-0006, 3.9

	10
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
(  )APROVADO      (  )REPROVADO

FINAL INSPECTION. ( )APPROVED ( )FAILED
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· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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