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	ITEM
(Item)
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	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	A-) REMOVER OS DOIS CAGES CENTRAIS ASSINALADOS.
B-) INSTALAR OS 3- PRISIONEIROS, DEIXANDO A ALTURA= 1.828¨
C-) PASSAR A BROCA FERRAMENTA NOS 4- FUROS PASSANTES.

A-) REMOVE THE TWO CENTRAL CAGES MARKED. B-) INSTALL THE 3- PRISONERS, LEAVING THE HEIGHT = 1.828 ̈ C-) PASS THE TOOL DRILL IN THE 4-THROUGH HOLES.

	2
	REPAIR SHOP	USINAGEM / MACHINING	USINAR OS DOIS ALOJAMENTOS DOS CAGES CENTRAIS REMOVIDOS, CENTRANDO PELOS PROPRIOS DIÂMETROS INTERNOS, ATÉ DESOVALIZA-LOS.
 PODE FICAR PEQUENA MANCHA.

MACHINE THE TWO REMOVED CENTRAL CAGE HOUSINGS, CENTERING BY THEIR OWN INTERNAL DIAMETERS, UNTIL THEY ARE DEVALUED. IT MAY BE A SMALL STAIN.

	3
	T56A	INSPEÇÃO / INSPECTION	CRIAR O.S. PARA CROMAR OS CAGES, JÁ DETERMINANDO A MEDIDA FINAL DOS MESMOS.

CREATE O.S. TO CHROME THE CAGES, ALREADY DETERMINING THEIR FINAL MEASUREMENT.

	4
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	5
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-A, LEVEL-3.
APRESENTOU INDICAÇÃO?   (  )SIM    (  )NÃO

RUN FPI: ASTM E 1417, METHOD-A, LEVEL-3. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	6
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	7
	REPAIR SHOP	ISOLAÇÃO / MASK	ISOLAR OS PRISIONEIROS, FUROS E AS ÁREAS DE CONTATO.

ISOLATE STUDS, HOLES, AND CONTACT AREAS.

	8
	REPAIR SHOP	PINTURA / PAINTING	PINTAR EXTERNAMENTE COM:
PRIMER PA-0060
e CINZA PA-0065

PAINT EXTERNALLY WITH: PRIMER PA-0060 and GREY PA-0065

	9
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	REMOVER AS ISOLAÇÕES E OS EXCESSOS.

REMOVE INSULATION AND EXCESSES.

	10
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	INSTALAR OS CAGES E FRENA-LOS COM PINOS P/N= 17341

INSTALL THE CAGES AND BRAKE THEM WITH P/N PINS = 17341

	11
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
(  )APROVADO       (  )REPROVADO

FINAL INSPECTION. ( )APPROVED ( )FAILED
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· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)


	




image1.png




