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	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	AE- 109008
	     BRAKE OUTER MEMBER
	REVISÃO GERAL / OVERHAUL	1

	
	
	
	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	CHEMICAL CLEANING	LIMPAR / CLEAN	REMOVER O LINING E 
POLIR O DIÂMETRO INTERNO DO MEMBER, ONDE SE INSTALARÁ O NOVO LINING.

REMOVE THE LINING AND POLISH THE INNER DIAMETER OF THE MEMBER, WHERE THE NEW LINING WILL BE INSTALLED.

	2
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	MONTAR O NOVO LINING, AJUSTANDO-O E PRENDENDO COM 24 NOVOS REBITES P/N= MS20427-3C5
VEJA A PROFUNDIDADE INDICADA NA FIGURA ANEXA.

ASSEMBLE THE NEW LINING, ADJUSTING IT AND SECURING IT WITH 24 NEW RIVETS P/N= MS20427-3C5 SEE THE DEPTH INDICATED IN THE ATTACHED FIGURE.

	3
	CHEMICAL CLEANING	LIMPAR / CLEAN	USINAR O DIÂMETRO INTERNO DO LINING, DEIXANDO DENTRO DOS LIMITES DO GABARITO P/N=6796436

MACHINE THE INNER DIAMETER OF THE LINING, LEAVING IT WITHIN THE LIMITS OF THE TEMPLATE P/N=6796436

	4
	REPAIR SHOP	ISOLAÇÃO / MASK	USINAR NOVOS 24 RASGOS NO DIÂMETRO INTERNO DO LINING, NO CENTRO DE CADA ESPAÇO DOS REBITES, MEDIDAS: 0.100¨-0.007¨ DE LARGURA e 0.013¨+ou- 0.002¨ DE PROFUNDIDADE.

MACHINE NEW 24 SLOTS IN THE INNER DIAMETER OF THE LINING, IN THE CENTER OF EACH RIVET SPACE, MEASURES: 0.100 ̈-0.007 ̈ WIDTH and 0.013 ̈+or- 0.002 ̈ DEPTH.

	5
	REPAIR SHOP	PINTURA / PAINTING	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	6
	REPAIR SHOP	Escolher um item.	EXECUTAR MPI: ASTM E 1444.
APRESENTOU INDICAÇÃO? (  )SIM   (  )NÃO 

RUN MPI: ASTM E 1444. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	7
	T56A	Escolher um item.	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	8
	Escolher um item.	Escolher um item.	INSPEÇÃO FINAL.
 (  ) APROVADO   (  )REPROVADO

FINAL INSPECTION. ( ) APPROVED ( )FAILED

	
	Escolher um item.	Escolher um item.	
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(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 31/10/2025
(Date):

	[bookmark: Texto2]     
	VILSON BARBOSA
	31/10/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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