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	TLN: 02188

	                      23006662
	                           15446
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	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	T56  -  IAS
	1- PUMP COVER
	REVISÃO GERAL / OVERHAUL	1

	
	
	
	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	REMOVER A BUCHA DE BRONZE.

REMOVE BRONZE BUSHING.

	2
	CHEMICAL CLEANING	DECAPAGEM / STRIPPING	DECAPAR A TINTA, CONFORME A IP-0006, 3.18

INK PICKLING, IN ACCORDANCE WITH IP-0006, 3.18

	3
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	4
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-A, LEVEL-3.
APRESENTOU INDICAÇÃO?   ( )SIM    ( )NÃO

RUN FPI: ASTM E 1417, METHOD-A, LEVEL-3. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	5
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10


	6
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	MONTAR A BUCHA E FRENAR COM O PINO P/N= AN150306
VEJA A FIGURA ANEXA.

MOUNT THE BUSHING AND BRAKE WITH P/N= AN150306 SEE THE ATTACHED FIGURE.

	7
	REPAIR SHOP	USINAGEM / MACHINING	USINAR O DIÂMETRO INTERNO DA BUCHA, DEIXANDO= 0.5007¨+ou- 0.0002¨
CHANFRAR , DEIXANDO A BUCHA NO MESMO PLANO DA FACE OU LEVEMENTE A BAIXO.
     VEJA A FIGURA ANEXA.
MACHINE THE INNER DIAMETER OF THE BUSHING, LETTING= 0.5007 ̈ + or - 0.0002 ̈ CHAMFER, LEAVING THE ANCHOR IN THE SAME PLANE AS THE FACE OR SLIGHTLY BELOW. SEE THE ATTACHED FIGURE.

	8
	REPAIR SHOP	ISOLAÇÃO / MASK	ISOLAR OS FUROS E A FACE DE CONTATO.
ISOLATE THE HOLES AND THE CONTACT FACE.

	9
	REPAIR SHOP	PINTURA / PAINTING	PINTAR EXTERNAMENTE COM:
PRIMER PA-0060 e CINZA PA-0065.

PAINT EXTERNALLY WITH: PRIMER PA-0060 and GRAY PA-0065.

	10
	REPAIR SHOP	REMOVER ISOLAMENTO / REMOVE MASK	REMOVER AS ISOLAÇÕES E OS EXCESSOS DE TINTA.

REMOVE INSULATION AND EXCESS PAINT.

	11
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
( )APROVADO       ( )REPROVADO

FINAL INSPECTION. ( )APPROVED ( )FAILED

	
	Escolher um item.	Escolher um item.	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 24/06/2026
(Date):

	[bookmark: Texto2]     
	VILSON BARBOSA
	24/06/2026


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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