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	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:

	3045348-01
	RGM-AX0093
	INSERIR NA O.S 054346
	01509

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE
(Article/Part):
	Serviço Principal
(Main Service):
	QUANT:


	PCE-AX0093
	COMPLETE ENGINE ASSEMBLY
	REPARO / REPAIR	1

	TSN:
	CSN:
	TSO:
	CSO:

	ITEM
(Item)
	TAREFA
(Task)
	ETAPA
(Step)
	DESCRIÇÃO
(Description)

	01
	CTM
	ANALISE INICIAL DE DOCUMENTAÇÃO / INITIAL DOCUMENTATION ANALYSIS	
Verificar se o escopo está em conformidade com a revisão mais recente do manual aplicável. Para isso, conferir se a revisão mencionada abaixo corresponde à revisão vigente do manual disponível, conforme localização mencionada na Intranet:

Conforme Overhaul Manual_ 3044823 _ Rev. 31 17 Nov. 2025.

(Verify that the scope complies with the latest revision of the applicable manual. To do so, check whether the revision indicated below matches the current revision of the manual available, as per the location specified on the Intranet:)

According to Overhaul Manual_ 3044823 _ Rev. 31 17 Nov. 2025.)

Nota: caso haja divergência, não seguir com as próximas etapas e notificar de forma imediata via e-mail a Engenharia para que seja realizada a atualização do escopo.
(Note: if there is any discrepancy, do not proceed with the following steps and immediately notify the Engineering team responsible by email so that the scope can be updated accordingly.)


	02
	PW100	DESMONTAGEM / DISASSEMBLY	
Realizar a remoção da Accessory Drive Cover e  Gearshaft Assemblies, conforme OVH 3044823, ATA 72-10-00, Seção “Disassembly”, Parágrafo 5., Etapa A., B., C., D. , Figura 101.
(Perform removal of the Accessory Drive Cover and Gearshaft Assemblies in accordance with OVH 3044823, ATA 72-10-00, Section “Disassembly”, Paragraph 5, Steps A, B, C, and D, Figure 101.)


	03
	PW100	DESMONTAGEM / DISASSEMBLY	
Realizar a remoção da Input Drive Housing Assembly, conforme OVH 3044823, ATA 72-10-00, Seção “Disassembly”, Parágrafo 6. , Figura 102.
(Perform removal of the Input Drive Housing Assembly in accordance with OVH 3044823, ATA 72-10-00, Section “Disassembly”, Paragraph 6, Figure 102.)

	04
	PW100	DESMONTAGEM / DISASSEMBLY	
Realizar a remoção da First-stage Reduction Gears, conforme OVH 3044823, ATA 72-10-00, Seção “Disassembly”, Parágrafo 7. , Etapa A., Figura 103.
(Perform removal of the First-Stage Reduction Gears in accordance with OVH 3044823, ATA 72-10-00, Section “Disassembly”, Paragraph 7, Step A, Figure 103.)


	05
	PW100	DESMONTAGEM / DISASSEMBLY	
Realizar a remoção da Front Housing Assembly, conforme OVH 3044823, ATA 72-10-00, Seção “Disassembly”, Parágrafo 8. , Etapa A. e B., Figura 104.
(Perform removal of the Front Housing Assembly in accordance with OVH 3044823, ATA 72-10-00, Section “Disassembly”, Paragraph 8, Steps A and B, Figure 104.)


	06
	PW100	INSPEÇÃO / INSPECTION	
Realizar inspeção visual da Reduction Gearbox aberta em 3 partes conforme orientação da Pratt e Whitney em consulta aberta para o caso. 
(Perform a visual inspection of the Reduction Gearbox (RGB) disassembled into three sections, in accordance with guidance provided by Pratt & Whitney through the open technical inquiry related to this case.)

Foi localizado a discrepância? 
(Was the discrepancy identified?)

(   ) Sim.
       (Yes.)

(   ) Não.
       (No.)

Caso seja encontrada alguma discrepância ou dano, é mandatória a descrição e registros fotográficos utilizando o formulário IAS-RG-0007 – Relatório de Trabalho.
(If any discrepancy or damage is found, a description and photographic records using form IAS-RG-0007 – Work Report is mandatory.)


	07
	PW100	LIMPAR / CLEAN	
Realizar o envio dos injetores de óleo para Pressure Flush. 
(Perform shipment of the oil nozzles for pressure flushing.)


	08
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a instalação dos Plain Plugs, Machine Plugs, Oil Nozzles and Covers na Rear Housing Assembly, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-1”, Parágrafo 7. , Etapa B., Figura 506.
(Perform installation of the Plain Plugs, Machine Plugs, Oil Nozzles, and Covers on the Rear Housing Assembly, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-1”, Paragraph 7, Step B, Figure 506.)

	09
	PW100	MONTAG EM/ ASSEMBLY	Realizar a instalação dos Borescope Covers na Rear Housing Assembly, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-1”, Parágrafo 7. , Etapa C., Figura 506.
(Perform installation of the Borescope Covers on the Rear Housing Assembly, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-1”, Paragraph 7, Step C, Figure 506.)


	10
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a instalação dos Transfer Tubes and Layshaft Bearing Oil Nozzles na Rear Housing Assembly, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-1”, Parágrafo 8. , Etapa B., Figura 509.
(Perform installation of the Transfer Tubes and Layshaft Bearing Oil Nozzles on the Rear Housing Assembly, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-1”, Paragraph 8, Step B, Figure 509)


	11
	PW100	MONTAG EM/ ASSEMBLY	
Realizar o acoplamento da Rear Housing Assembly e Front Housing Assembly, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-1”, Parágrafo 8. , Etapa C., Figura 509.
(Perform mating of the Rear Housing Assembly and Front Housing Assembly, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-1”, Paragraph 8, Step C, Figure 509.)


	12
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a montagem do Input Shaft, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-1”, Parágrafo 10. , Etapa B., Figura 510.
(Perform installation of the Input Shaft, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-1”, Paragraph 10, Step B, Figure 510.)

PN do Input Shaft: ______________________
(Input Shaft P/N:)

SN do Input Shaft: ______________________
(Input Shaft S/N:)

PN do Rolamento Nº 8. (Traseiro) : _____________________
(No. 8 Bearing P/N (Rear):)

SN do Rolamento Nº 8. (Traseiro): _____________________
(No. 8 Bearing S/N (Rear):)

PN do Rolamento Nº 9. (Frontal): _____________________
(No. 9 Bearing P/N (Rear):)

SN do Rolamento Nº 9. (Frontal): _____________________
(No. 9 Bearing S/N (Rear):)



	13
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a montagem das pistas externas do No. 8 and 11 Bearing, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-1”, Parágrafo 11., Etapa D., Figura 511.
(Perform installation of the No. 8 and No. 11 Bearing Outer Races, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-1”, Paragraph 11, Step D, Figure 511.)


	14
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a instalação das Layshafts and Input Shaft, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-1”, Parágrafo 11., Etapa C., Figura 510.
(Perform installation of the Layshafts and Input Shaft, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-1”, Paragraph 11, Step C, Figure 510.)


	15
	PW100	MONTAG EM/ ASSEMBLY	
Realizar o acoplamento das Housing, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-1”, Parágrafo 11., Etapa D., Figura 510.
(Perform mating of the Housing Assemblies, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-1”, Paragraph 11, Step D, Figure 510.)

	16
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a instalação dos Oil Nozzles, Transfer Tube and Gearshafts in Rear Housing, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-2”, Parágrafo 5., Etapa E.
(Perform installation of the Oil Nozzles, Transfer Tube, and Gearshafts in the Rear Housing, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-2”, Paragraph 5, Step E.)


	17
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a instalação da Accessory Drive Cover on Rear Housing, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-2”, Parágrafo 5., Etapa F.
(Perform installation of the Accessory Drive Cover on the Rear Housing, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-2”, Paragraph 5, Step F.)


	18
	PW100	MONTAG EM/ ASSEMBLY	
Realizar o acoplamento Venier, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-2”, Parágrafo 6., Etapa A. e B., Figura 503.
(Perform Vernier coupling in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-2”, Paragraph 6, Steps A and B, Figure 503.)


	19
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a instalação dos Layshaft Covers, Nipple and Elbow, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-2”, Parágrafo 7., Etapa B., Figura 504.
(Perform installation of the Layshaft Covers, Nipple, and Elbow, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-2”, Paragraph 7, Step B, Figure 504.)


	20
	PW100	MONTAG EM/ ASSEMBLY	
Realizar a instalação Input Shaft Drive Coupling, conforme OVH 3044823, ATA 72-10-00, Seção “Sub-Assembly-2”, Parágrafo 8., Etapa A e B., Figura 505.
(Perform installation of the Input Shaft Drive Coupling, in accordance with OVH 3044823, ATA 72-10-00, Section “Sub-Assembly-2”, Paragraph 8, Steps A and B, Figure 505.)

(ref. Parágrafo 8 (B))
(ref. Paragraph 8 (B))

Dimensão C: ___________ [in]
(Dimension C:)


	21
	PW100	INSPEÇÃO / INSPECTION	
Realizar a inspeção final do serviço realizado. 

(Perform final inspection of the service performed.)

	
	
	
	

	OBSERVAÇÕES (REMARKS):
	ASSINATURA DO SOLICITANTE (Signature):
	DATA (Date):

	
O.S. solicitada para realização de abertura Reduction Gearbox (RGB) conforme orientação da Pratt e Whitney, após pico de Vibração dela no teste final pós pesquisa de pane do ruído anormal, montagem após tratativa da pane na RGB, teste e preservação do motor. 
(Work Order requested to perform the disassembly of the Reduction Gearbox (RGB) in accordance with Pratt & Whitney's recommendation, following an RGB vibration peak observed during the final test after troubleshooting of the abnormal noise. The Work Order also includes reassembly following corrective action on the RGB, engine testing, and engine preservation.)
	
	25/06/2026


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department.)


image1.png




