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	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
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	SUPPLEMENTARY REQUEST
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	P/N:
	S/N:
	O.S.: (W.O.):
	TLN:

	022489-054-03
	5995
	039498
	TLN02361

	Nº DO ARTIGO PRINCIPAL: (Main Article No.):
	ARTIGO/PARTE (Article/Part):
	QUANT:

	AE-109928
	DUAL GEAR TYPE FUEL PUMP WITH BOOSTER
	01

	TSN: UNK
	CSN: UNK
	TSO: UNK
	CSO: UNK

	Conforme OHM With IPL _ UTC Aerospace Systems _ 73-1-2
(According to OHM With IPL _ UTC Aerospace Systems _ 73-1-2)

	ITEM
(Item)
	DESCRIÇÃO DO SERVIÇO A EXECUTAR
 (Description of the work to be executed)
	EXECUÇÃO
(Execution)
	*SETOR/FORNECEDOR
(Sector/Supplier)

	01
	Realizar inspeção de recebimento do item, analisando danos e discrepâncias externas. Caso seja encontrada alguma discrepância ou dano, é mandatória a descrição e registros fotográficos utilizando o formulário IAS-RG-0007 – Relatório de Trabalho.

Perform receipt inspection of the item, analyzing external damage and discrepancies. If any discrepancy or damage is found, a description and photographic records using form IAS-RG-0007 – Work Report is mandatory.
	
	Acessórios

Accessories

	02
	Realizar teste inicial do item, conforme seções “Testing” e “Troubleshooting” itens 1 a 4 e 1 e 2, respectivamente. Preencher ficha de teste do manual (figura 704, página 706 e 707) indicando que se refere ao teste inicial.

Caso seja encontrada alguma discrepância ou dano, é mandatória a descrição e registros fotográficos utilizando o formulário IAS-RG-0007 – Relatório de Trabalho. Solicite sub O.S.’s conforme necessário para correção utilizando o formulário IAS-RG-0103 – Solicitação de Serviços Complementares.

Perform the inicial test of the item, according to sections “Testing” and “Troubleshooting” items 1 to 4 and 1 and 2, respectively. Complete the test form in the manual (figure 704, pages 706 and 707) indicating that it refers to the inicial test.

If any discrepancy or damage is found, a description and photographic records using the form IAS-RG-0007 – Work Report is mandatory. Request sub W.O.s as necessary for correction using form IAS-RG-0103 – Supplementary Request.
	
	Acessórios

Accessories

	03
	Se necessário, realizar reparos e trocas necessárias no item, conforme seção “Repair” itens 1 e 2. Solicite sub O.S.’s conforme necessário utilizando o formulário IAS-RG-0103 – Solicitação de Serviços Complementares.

If necessary, perform repairs and necessary replacements on the item, according to section “Repair”, items 1 and 2. Request sub W.O.s as necessary using form IAS-RG-0103 – Supplementary Request.
	
	Acessórios

Accessories

	04
	Realizar teste final do item, conforme seções “Testing” e “Troubleshooting” itens 1 a 4 e 1 e 2, respectivamente. Preencher ficha de teste do manual (figura 704, página 706 e 707) indicando que se refere ao teste final. Caso seja encontrada alguma discrepância ou dano, é mandatória a descrição e registros fotográficos utilizando o formulário IAS-RG-0007 – Relatório de Trabalho.

Perform the final test of the item, according to sections “Testing” and “Troubleshooting” items 1 to 4 and 1 and 2, respectively. Complete the test form in the manual (figure 704, pages 706 and 707) indicating that it refers to the final test. If any discrepancy or damage is found, a description and photographic records using the form IAS-RG-0007 – Work Report is mandatory.
	
	Acessórios

Accessories

	05
	Inspeção final.

Final inspection.
	
	Acessórios

Accessories
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· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department).
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