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	REGISTRO
	REVISÃO
	1

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN(PN):
	SN:
	ARTIGO/PARTE(Article/Part):
	QUANT:
	TLN:
	Nº da OS(WO):

	362531-1
	0084LK
	QEC ASSY
	1
	TO 1C-130A-3
	038098

	ITEM
(Item)
	DESCRIÇÃO DO SERVIÇO A EXECUTAR
(Description of thework to be executed)
	EXECUÇÃO
(Execution)
	*SETOR/FORNECEDOR
(Sector/Supplier)

	
	 
REALIZAR INSPEÇÃO GERAL (TO 1C-130A-3 - ENGINE NACELLE - 54-20-00 (PDF 1535)) NAS PARTES DO QEC CONFORME ABAIXO CITADOS:
PERFORM GENERAL INSPECTION (TO 1C-130A-3 - ENGINE NACELLE - 54-20-00 (PDF 1535)) ON THE QEC PARTS AS LISTED BELOW:


NACELLE DO Q.E.C
PORTAS DE ACESSO SUPERIORES
PORTAS DE ACESSO INFERIORES
TAMPAS DE ACESSO
CARENAGEM FRONTAL (BOCAL DE ENTRADA)
CARENAGEM SUPERIOR
CARENAGEM INFERIOR (CANOA)
Q.E.C NACELLE
UPPER ACCESS DOORS
LOWER ACCESS DOORS
ACCESS COVERS
FRONT FAIRING (INTAKE PLUG)
UPPER FAIRING
LOWER FAIRING (CANOE)

INSPECIONAR CONTRA CORROSÃO TODAS AS SUPERFICIES; INSPECIONAR TODOS OS DIZUS CONTRA CORROSSÃO E DANOS;
INSPECIONAR TRAVAS E ALOJAMENTOS DOS DIZUS;
INSPECIONAR QUANTO REBITES TRABALHANDO;
INSPECIONAR QUANTO REBITES FLUTUANDO;
INSPECIONAR QUANTO A DANOS E AMASSADOS INTERNOS; INSPECIONAR QUANTO A DANOS E AMASSADOS EXTERNOS; INSPECIONAR QUANTO A DESGASTES INTERNOS E EXTERNOS;
 
 INSPECT ALL SURFACES FOR CORROSION; INSPECT ALL DIZUS FOR CORROSSION AND DAMAGE;
INSPECT DIZUS LOCKS AND HOUSINGS;
INSPECT FOR WORKING RIVETS;
INSPECT FOR FLOATING RIVETS;
INSPECT FOR INTERNAL DAMAGE AND DENTS; INSPECT FOR EXTERNAL DAMAGE AND DENTS; INSPECT FOR INTERNAL AND EXTERNAL WEAR;


TO 1C-130A-3 - ENGINE NACELLE - 54-20-00 (PDF 1535)


OBS: QUALQUER DÚVIDA CONSULTAR A ENGENHARIA IAS.
NOTE: FOR ANY QUESTIONS, CONSULT IAS ENGINEERING.

	
	


















REPAROS IAS

	
	EXECUTAR REPARO CONFORME NECESSÁRIO DENTRO DOS PARAMETROS DA TO 1C-130A-3 - ENGINE NACELLE - 54-20-00 

PERFORM REPAIR AS NECESSARY WITHIN PARAMETERS OF TO 1C-130A-3 - ENGINE NACELLE - 54-20-00

OBS: QUALQUER DÚVIDA DOS REPAROS CONSULTAR A ENGENHARIA IAS.
NOTE: FOR ANY QUESTIONS ABOUT REPAIRS, CONSULT IAS ENGINEERING.



	
	



REPAROS IAS

	
	EXECUTAR TRATAMENTO DE CORROSÃO EM TODAS AS SUPERFICIES ABAIXO:
PERFORM CORROSION TREATMENT ON ALL SURFACES BELOW:

NACELLE DO Q.E.C
PORTAS DE ACESSO SUPERIORES
PORTAS DE ACESSO INFERIORES
TAMPAS DE ACESSO
CARENAGEM FRONTAL (BOCAL DE ENTRADA)
CARENAGEM SUPERIOR
CARENAGEM INFERIOR (CANOA)
Q.E.C NACELLE
UPPER ACCESS DOORS
LOWER ACCESS DOORS
ACCESS COVERS
FRONT FAIRING (INTAKE PLUG)
UPPER FAIRING
LOWER FAIRING (CANOE)


OBS: QUALQUER DÚVIDA DO TRATAMENTO CONSULTAR A ENGENHARIA IAS.
NOTE: FOR ANY QUESTIONS ABOUT THE TREATMENT, CONSULT IAS ENGINEERING.

	
	








REPAROS IAS

	
	ISOLAR AREAS ADJACENTES E EXECUTAR PINTURA INTERNA E EXTERNA CONFORME ‘’TINTAS DEFINIDAS PELA ENGENHARIA IAS’’ NAS SUPERFICIES ABAIXO:
ISOLATE ADJACENT AREAS AND PERFORM INTERNAL AND EXTERNAL PAINTING IN ACCORDANCE WITH ‘’PAINTS DEFINED BY IAS ENGINEERING’’ ON THE SURFACES BELOW:

NACELLE DO Q.E.C
PORTAS DE ACESSO SUPERIORES
PORTAS DE ACESSO INFERIORES
TAMPAS DE ACESSO
CARENAGEM FRONTAL (BOCAL DE ENTRADA)
CARENAGEM SUPERIOR
CARENAGEM INFERIOR (CANOA)
Q.E.C NACELLE
UPPER ACCESS DOORS
LOWER ACCESS DOORS
ACCESS COVERS
FRONT FAIRING (INTAKE PLUG)
UPPER FAIRING
LOWER FAIRING (CANOE)


OBS: QUALQUER DÚVIDA DA PINTURA CONSULTAR A ENGENHARIA IAS.
NOTE: FOR ANY QUESTIONS ABOUT PAINTING, CONSULT IAS ENGINEERING.

	
	










PINTURA

	
	REMOVER ISOLAÇÕES E EXCESSOS, E LIMPAR COM AR COMPRIMIDO
REMOVE INSULATION AND EXCESS, AND CLEAN WITH COMPRESSED AIR

	
	PINTURA

	
	INSPEÇÃO FINAL

FINAL INSPECTION.




	
	INSPEÇÃO

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA
(Date):

	 
TO 1C-130A-3 - ENGINE NACELLE 

NACELLE/PYLON REPAIRS - 54-10-00 (PDF 1531)
ENGINE NACELLE - 54-20-00 (PDF 1535)

	ANDRÉ
	
22/11/2024



· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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