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	RECORD
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	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:02623

	            6854716
	RWY25643
	039483
	

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	MÉXICO  /  CAE-550449  /  D22A
	1- WHEEL 6º ST
	REVISÃO GERAL / OVERHAUL	1

	
	
	
	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	REMOVER PALHETAS / REMOVE BLADES	REMOVER TODAS AS PALHETAS REFUGOS, MARCADAS DE VERMELHO,
ENSACA-LAS E DEVOLVER SEPARADAS PARA A INSPEÇÃO.

REMOVE ALL SCRAP VANES, MARKED RED, BAG THEM AND RETURN THEM SEPARATELY FOR INSPECTION.

	2
	REPAIR SHOP	REMOVER PALHETAS / REMOVE BLADES	REMOVER OS PEDAÇOS DE PINOS DA RODA.

REMOVE THE PIECES OF WHEEL PINS.

	3
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR A RODA, CONFORME A IP-0006, 3.8

CLEANING THE WHEEL IN ACCORDANCE WITH IP-0006, 3.8

	4
	NDT	END- PARTICULAS MAGNETICAS / NOT - MAGNETIC PARTICLE	EXECUTAR MPI: ASTM E 1444.
APRESENTOU INDICAÇÃO? (  )SIM        (  )NÃO

RUN MPI: ASTM E 1444. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	5
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	6
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-D, LEVEL-4.
APRESENTOU INDICAÇÃO? (  )SIM      (  )NÃO

RUN FPI: ASTM E 1417, METHOD-D, LEVEL-4. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	7
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	8
	CHEMICAL CLEANING	DEPOSIÇÃO DE NIQUEL-CADMIO / NICKEL-CADMIUM PLATING	APLICAR BANHO DE NICKEL CÁDMIO, 2416.

APPLY NICKEL CADMIUM BATH, 2416.

	9
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	MONTAR AS NOVAS PALHETAS E NÃO FRENA-LAS.

ASSEMBLE THE NEW BLADES AND DO NOT BRAKE THEM.

	10
	REPAIR SHOP	BALANCEAMENTO / BALANCING	CONFERIR E INFORMAR O PONTO E O VALOR DE DESBALANCEAMENTO.

CHECK AND INFORM THE POINT AND VALUE OF UNBALANCE.

	11
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	FRENAR AS PALHETAS COM PINOS P/N= 6730907 E EXECUTAR STAK.

BRAKE THE VANES WITH P/N 6730907 PIN AND PERFORM STAK.

	12
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
(  )APROVADO       (  )REPROVADO

FINAL INSPECTION. ( )APPROVED ( )FAILED

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 27/03/2025
(Date):

	[bookmark: Texto2]     
	VILSON BARBOSA
	27/03/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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