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	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:
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	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	AE-106837                   
	ACCESSORY DRIVE HOUSING ASSY
	REVISÃO GERAL / OVERHAUL	1

	TSN:
	CSN:
	TSO:
	CSO:

	Conforme Overhaul Manual for T56-A-15LFE _ 15RC3 _ 72-63-00 
(According to Overhaul Manual for T56-A-15LFE _ 15RC3 _ 72-63-00)

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	T56A	INSPEÇÃO PRELIMINAR/ PRELIMINARY INSPECTION	
Realizar inspeção de recebimento do Accessory Drive Housing Assy, analisando danos e discrepâncias externas. Caso seja encontrada alguma discrepância ou dano, é mandatória a descrição e registros fotográficos utilizando o formulário IAS-RG-0007 – Relatório de Trabalho.

Perform receipt inspection of the Accessory Drive Housing Assy, analyzing external damage and discrepancies. If any discrepancy or damage is found, a description and photographic records using form IAS-RG-0007 – Work Report is mandatory.


	2
	T56A	DESMONTAGEM / DISASSEMBLY	
Realizar a desmontagem da Accessory Drive Housing Assy, conforme Overhaul Manual for 501-D22A _ 4RC3 _ 72-63-00.

Dismantle the Accessory Drive Housing Assy in accordance with the Overhaul Manual for 501-D22A _ 4RC3 _ 72-63-00.


	3
	CHEMICAL CLEANING	LIMPAR / CLEAN	
Realizar a limpeza dos componentes da Accessory Drive Housing Assy, conforme Overhaul Manual for 501-D22A _ 4RC3 _ 72-63-01/ 72-63-03/ 72-63-09/ 72-63-11/ 72-63-15/72-63-17/72-63-19.

Clean the Accessory Drive Housing Assy components in accordance with the Overhaul Manual for 501-D22A _ 4RC3 _ 72-63-01/ 72-63-03/ 72-63-09/ 72-63-11/ 72-63-15/72-63-17/72-63-19.


	4
	T56A	INSPEÇÃO / INSPECTION	
Realizar inspeção do item a nível overhaul, bem como reparos e trocas necessárias, conforme manual.

Caso seja encontrada alguma discrepância, é mandatória a descrição e registros fotográficos utilizando o formulário IAS-RG-0007 – Relatório de Trabalho. Solicite sub O.S.’s conforme necessário utilizando o formulário IAS-RG-0103 – Solicitação de Serviços Complementares.

Perform inspection of the item at overhaul level, as well as necessary repairs and replacements, according to manual.

If any discrepancy is found, a description and photographic records using the form IAS-RG-0007 – Work Report is mandatory. Request sub W.O.s as necessary using form IAS-RG-0103 – Supplementary Request.


	5
	T56A	MONTAG EM/ ASSEMBLY	
Realizar a montagem da Accessory Drive Housing Assy, conforme Overhaul Manual for 501-D22A _ 4RC3 _ 72-63-00.

Assemble the Accessory Drive Housing Assy in accordance with the Overhaul Manual for 501-D22A _ 4RC3 _ 72-63-00.


	
	T56A	INSPEÇÃO / INSPECTION	
Inspeção final.

Final inspection.


	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
(Date):
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	GUILHERME BRAGA
	05/05/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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