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	REGISTRO
	REVISÃO
	02

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:

	RR30000453
	N/C
	044489
	2027

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	QUANT:

	RRE-200214
	LINER
	01

	TSN:                           UNK
	CSN:         UNK
	TSO:               UNK 
	CSO:                 UNK

	ITEM
(Item)
	DESCRIÇÃO DO SERVIÇO A EXECUTAR
 (Description of the work to be executed)
	EXECUÇÃO
(Execution)
	*SETOR/FORNECEDOR
(Sector/Supplier)

	01
	REALIZAR AJUSTE DAS FLAUTAS PARA UMA ABERTURA QUE PODE VARIAR DE 0.050-0.070 in. (1.27-1.78 mm) CONFORME HMM-CSP22005.

MAKE ADJUSTMENT OF THE FLUTES FOR AN OPENING THAT CAN VARY FROM 0.050-0.070 in. (1.27-1.78 mm) ACCORDING TO HMM-CSP22005.
	
	REPAROS

	02
	INSPEÇÃO FINAL

FINAL INSPECTION
	
	INSPEÇÃO

	03
	
	
	

	04
	
	
	

	05
	
	
	

	06
	
	
	

	07
	
	
	

	08
	
	
	

	09
	
	
	

	10
	
	
	

	
	
	
	

	
	
	
	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
(Date):

	[bookmark: Texto2]     
	ANTONIO CLAUDIO
	04/06/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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