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	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:

	RR30000332
	JY105175
	044639
	02027

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	RR300 / RRE-200280
	Impeller
	REPARO / REPAIR	01 EA

	TSN:
	CSN:
	TSO:
	CSO:

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	Realizar polimento do bordo de ataque utilizando lixa grão 1200.
NOTA: REALIZAR POLIMENTO MANUALMENTE, NÃO UTILIZAR EQUIPAMENTOS ROTATIVOS. ELETRICOS, PNEUMATICOS, ETC.

Polish leading edge with sandpaper grit 1200.
POLISHING MUST BE DONE MANUALLY. THE USE OF ROTARY EQUIPMENT IS NOT PERMITTED. (E.G., ELECTRIC OR PNEUMATIC TOOLS).

	2
	RR300	INSPEÇÃO / INSPECTION	Inspeção final

Final inspection.

	
	
	
	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
(Date):

	[bookmark: Texto2]     
	Patrick Dimas
	23/06/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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