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	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:

	6875121
	                      TS0175A
	               45000
	2188

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	---
	LEVER, FUEL CUTOFF OUTPUT
	REPARO / REPAIR	4

	TSN:
	CSN:
	TSO:
	CSO:

	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	02
	CHEMICAL PROCESS
	LIMPEZA
	Realize a decapagem do componente em acordo a IAS-IT-0273

Perform component stripping in accordance with IAS-IT-0273.

	03
	CHEMICAL PROCESS
	APLICAÇÃO
	Realize a aplicação do revestimento do componente em acordo a TASK 70-01-11-300-801 (Cadmium Touch-up Plating Maintenance Practices) do manual de TLN 02188, página 75.

Apply the component coating in accordance with TASK 70-01-11-300-801 (Cadmium Touch-up Plating Maintenance Practices) in the TLN 02188 manual, page 75.

OBS: APLICAR BANHO DE CÁDMIO COM CROMATO
NOTE: APPLY CADMIUM PLATING WITH CHROMATE

	04
	ACESSÓRIOS
	INSPEÇÃO
	Realizar inspeção do componente a fim de garantir que a aplicação do “coating” está adequada.

Inspect the component to ensure that the coating has been applied properly.

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
(Date):

	Juntamente do LEVER, acompanha para serviço os seguintes itens:
Along with the LEVER, the following items are included for service:

Lever, Condition – PN 6812634
Pointer, Coordinator – PN 6812620
Cap, Coordinator – PN 6812619
Lever, Coordinator, Prop Setting – PN 6814486
	Arthur Castro
	25/08/25


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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