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	PN (PN):
	SN:
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	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	AE- 109024
	TU. FRONT BEARING SUPPORT
	REVISÃO GERAL / OVERHAUL	1

	
	
	
	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	RETIFICA / RECTIFY	PRENDER PELO DIÂMETRO ¨A¨ e RETIFICAR OS DIÂMETROS: F= 4.756¨e o C=9.2495¨
CENTRAR PELO DIÂMETRO ¨B¨ e a FACE ¨H¨
REMOVER CANTOS VIVOS.
VEJA A FIGURA ANEXA.

FASTEN BY DIAMETER ̈A ̈ and GRIND THE DIAMETERS: F= 4.756 ̈ and C=9.2495 ̈ CENTERING BY DIAMETER ̈B ̈ and FACE ̈H ̈ REMOVE SHARP CORNERS. SEE THE ATTACHED FIGURE.

	2
	REPAIR SHOP	RETIFICA / RECTIFY	ANTES DE DESPRENDER, APROVEITANDO AS CENTRAGENS, RETIFICAR A FACE ¨G¨, DEIXANDO MANCHAS, APENAS PARA ELIMINAR AS REBARBAS DE CROMO.
REMOVER CANTOS VIVOS.

BEFORE DETACHING, TAKING ADVANTAGE OF THE CENTRATIONS, RECTIFY THE ̈G ̈ FACE, LEAVING STAINS, JUST TO REMOVE THE CHROME BURRS. REMOVE SHARP CORNERS.

	3
	REPAIR SHOP	RETIFICA / RECTIFY	RETIFICAR A FACE ¨E¨, DEIXANDO A LARGURA COM A FACE- G= 0.864¨+ou- 0.0005¨
DEIXAR PARALELA COM AS FACES: D, G e H.
REMOVER CANTOS VIVOS.

LEAVE PARALLEL WITH THE FACES: D, G and H. REMOVE SHARP CORNERS.

	4
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	5
	NDT	END- PARTICULAS MAGNETICAS / NOT - MAGNETIC PARTICLE	EXECUTAR MPI: ASTM E 1444.
APRESENTOU INDICAÇÃO? (  )SIM      (  )NÃO

RUN MPI: ASTM E 1444. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	6
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	7
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
(  )APROVADO     (  )REPROVADO

FINAL INSPECTION. ( )APPROVED ( )FAILED

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 04/09/2025
(Date):

	[bookmark: Texto2]     
	VILSON BARBOSA
	04/09/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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