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	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
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	SUPPLEMENTARY REQUEST
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	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:02188

	                  6854756
	WY14781
	IAS
	

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	AE- 108598
	  COMPRESSOR WHEEL 6° ST.
	REVISÃO GERAL / OVERHAUL	1

	
	
	
	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	REMOVER TODOS OS PEDAÇOS DE PINOS.

REMOVE ALL PIECES OF PINS.

	2
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.8

CLEAR AS PER IP-0006, 3.8

	3
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-D, LEVEL-4.
APRESENTOU 

RUN FPI: ASTM E 1417, METHOD-D, LEVEL-4. PRESENTED

	4
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	5
	NDT	END- PARTICULAS MAGNETICAS / NOT - MAGNETIC PARTICLE	EXECUTAR MPI: ASTM E 1444.
APRESENTOU INDICAÇÃO? (  )SIM    (  )NÃO

RUN MPI: ASTM E 1444. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	6
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	7
	CHEMICAL CLEANING	DEPOSIÇÃO DE NIQUEL-CADMIO / NICKEL-CADMIUM PLATING	APLICAR BANHO DE NICKEL CÁDMIO, AMS 2416.

APPLY NICKEL CADMIUM BATH, AMS 2416.

	8
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	
INSTALAR AS PALHETAS, MAS NÃO FRENA-LAS.

INSTALL THE VANES, BUT DO NOT BRAKE THEM.

	9
	REPAIR SHOP	BALANCEAMENTO / BALANCING	
CONFERIR E INFORMAR O PONTO E O VALOR DO DESBALANCEAMENTO.

CHECK AND INFORM THE POINT AND VALUE OF THE UNBALANCE.

	10
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	FRENAR AS PALHETAS COM OS PINOS P/N= 6730907 E EXECUTAR STAK.

BRAKE THE VANES WITH THE PINS P/N= 6730907 AND PERFORM STAK.

	11
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
(  )APROVADO     (  )REPROVADO


FINAL INSPECTION. ( )APPROVED ( )FAILED

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 02/10/2025
(Date):

	[bookmark: Texto2]     
	VILSON BARBOSA
	02/10/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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