

	[image: Logotipo

Descrição gerada automaticamente]
	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
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	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	-
	TURBINE ASSY
	INSPEÇÃO / INSPECTION	01

	TSN:
	CSN:
	TSO:
	CSO:

	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	01
	M250
	DESMONTAGEM
	Realizar desmontagem da turbina e combustão para acesso a ‘GAS PRODUCER ROTOR ASSEMBLY’ em acordo a seção DISASSEMBLY, TASK 72-50-00-000-801.

Disassemble the turbine and combustion chamber to access the GAS PRODUCER ROTOR ASSEMBLY in accordance with section DISASSEMBLY, TASK 72-50-00-000-801.

	02
	LIMPEZA QUIMICA
	LIMPEZA
	Realizar limpezas aplicáveis conforme tabela 1 da seção CLEANING, SUBTASK 72-50-00-150-001.

Perform applicable cleaning according to Table 1 in the CLEANING section, SUBTASK 72-50-00-150-001.

	03
	LIMPEZA QUIMICA
	NDT
	Realizar NDT conforme especificado na Seção 72-50-00 – Turbine Section, Inspection/Check, aos componentes aplicáveis.

Disassemble the turbine and combustion chamber to access the GAS PRODUCER ROTOR ASSEMBLY in accordance with section DISASSEMBLY, TASK TASK 72-50-00-000-801.

	04
	LIMPEZA
	LIMPEZA
	Realizar limpeza aplicáveis pós NDT conforme tabela 1 da seção CLEANING, SUBTASK 72-50-00-150-001.

Perform applicable post-NDT cleaning according to Table 1 in the CLEANING section, SUBTASK 72-50-00-150-001.

	05
	M250
	INSPEÇÃO
	Realizar inspeção do componente em acordo a eção 72-50-00 – Turbine Section, Inspection/Check, aos componentes aplicáveis.

Perform component inspection in accordance with Section 72-50-00 – Turbine Section, Inspection/Check, on applicable components.

	06
	M250
	REPARO
	Realizar os reparos aplicáveis da turbina conforme os procedimentos definidos na Seção 72-50-00 – Turbine Section, itens REPAIR-801 a REPAIR-814.

Perform applicable turbine repairs in accordance with the procedures defined in Section 72-50-00 – Turbine Section, items REPAIR-801 to REPAIR-814. 


	07
	M250
	MONTAGEM
	Realizar montagem da turbina em acordo a seção ASSEMBLY, TASK 72-50-00-400-802.

Assemble the turbine in accordance with section ASSEMBLY, TASK 72-50-00-400-802.


	08
	M250
	TESTE FINAL
	Realizar o teste final do item, conforme especificado na Seção TESTING-801, utilizando a Ficha de Serviço FS.1040. Ressalta-se que este procedimento corresponde ao teste final do motor.

Perform the final test of the item, as specified in Section TESTING-801, using Service Sheet FS.1040. It should be noted that this procedure corresponds to the final test of the engine.

NOTA: Em caso de discrepâncias apresentadas no teste final, favor evidenciar no formulário IAS-RG-0007 – Relatório de Trabalho, juntamente de justificativas e/ou evidências 

NOTE: In the event of any discrepancies in the final test, please provide justification and/or evidence on form IAS-RG-0007 - Work Report.


	09
	M250
	APROVAÇÃO FINAL
	Inspeção final

Final Inspection
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· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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