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	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:

	23085138-5
	NC
	048460
	02118

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	RR300/ RRE-201438
	ORIFICE, DIFFUSER VENT
	REPARO / REPAIR	01

	     
	     
	TSO:                    
	CSO:      

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	01
	REPAIR SHOP	RETIFICA / RECTIFY	RETIFICAR DIAMENTRO DO ORIFICIO CALIBRADO PARA 0.309" A 0.317" IN. (7.85 A 8.05 MM ) ATENDENDO MEDIDAS DO PN: 6874924-4.  PARA ATENDER ESPECIFICAÇÕES DE DESEMPENHO DO MOTOR EM BANCO DE PROVAS.

RECTIFY CALIBRATED HOLE DIAMETER TO 0.309" TO 0.317" IN. (7.85 TO 8.05 MM) COMPLYING WITH PN: 6874924-4 MEASUREMENTS. TO MEET ENGINE PERFORMANCE SPECIFICATIONS ON A TEST BENCH.

	02
	RR300	INSPEÇÃO / INSPECTION	EFETUAR INSPEÇÃO DO ORIFICIO CALIBRADO DO  DIFFUSER VENT ORIFICE SE ESTA DENTRO DAS MEDIDAS PARA O PN:6874924-5 SENDO ENTRE 0309"-0.317" IN. (7.85-8.05 MM).


MEDIDA ENCONTRADA:_________________   

INSPECT THE CALIBRATED ORIFICE OF THE DIFFUSER VENT ORIFICE TO SEE IF IT IS WITHIN THE MEASUREMENTS FOR PN: 6874924-4, BETWEEN 0.309"-0.317" IN. (7.85-8.05 MM).

MEASUREMENT FOUND: _________________
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	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
(Date):

	[bookmark: Texto2]     
	[bookmark: Texto3]RICARDO CICALA
	[bookmark: Texto4]21/10/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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