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	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:02188

	               6859603
	PSS115
	IAS
	

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	AE-109692
	TU. VANE 3º ST
	REVISÃO GERAL / OVERHAUL	1

	
	
	
	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	CHEMICAL CLEANING	LIMPAR / CLEAN	REMOVER OS SEALS CONFORME A IP-0006, 3.8

REMOVE SEALS IN ACCORDANCE WITH IP-0006, 3.8

	2
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-A, LEVEL-3.
APRESENTOU INDICAÇÃO?  (  )SIM     (  )NÃO

RUN FPI: ASTM E 1417, METHOD-A, LEVEL-3. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	3
	CHEMICAL CLEANING	JATEAR / BLAST	LIMPAR COM GLASS BEAD BAIXA PRESSÃO. IP-0006,3.26

CLEAN WITH LOW PRESSURE GLASS BEAD. IP-0006,3.26

	4
	CHEMICAL CLEANING	DEPOSIÇÃO DE NIQUEL-CADMIO / NICKEL-CADMIUM PLATING	APLICAR NICKEL CÁDMIO, CONFORME AMS 2416.

APPLY NICKEL CADMIUM IN ACCORDANCE WITH AMS 2416.

	5
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	APLICAR NAS EXTREMIDADES DAS ALHETAS COM O OUTER RING, ADJACENTE AOS 5- FUROS O MATERIAL: SCOTCH -WELD No. 2214 Hi-Temp EPOXY ADHESIVE.

APPLY TO THE ENDS OF THE FINS WITH THE OUTER RING, ADJACENT TO THE 5-HOLES THE MATERIAL: SCOTCH-WELD No. 2214 Hi-Temp EPOXY ADHESIVE.

	6
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	INSTALAR OS NOVOS SEALS CONFORME A IT-0051.

INSTALL THE NEW SEALS ACCORDING TO IT-0051.

	7
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
(  )APROVADO         (  )REPROVADO

FINAL INSPECTION. ( )APPROVED ( )FAILED

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 27/10/2025
(Date):

	[bookmark: Texto2]     
	VILSON BARBOSA
	27/10/2025


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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