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	PCE-AX0093
	HIGH PRESSURE TURBINE DISK BALANCING ASSY
	REPARO / REPAIR	1

	TSN: N/A
	CSN: N/A
	TSO: N/A
	CSO: N/A

	ITEM
(Item)
	TAREFA
(Task)
	ETAPA
(Step)
	DESCRIÇÃO
(Description)

	01
	CTM
	ANALISE INICIAL DE DOCUMENTAÇÃO / INITIAL DOCUMENTATION ANALYSIS	
Verificar se o escopo está em conformidade com a revisão mais recente do manual aplicável. Para isso, conferir se a revisão mencionada abaixo corresponde à revisão vigente do manual disponível, conforme localização mencionada na Intranet:

Conforme Overhaul Manual_ 3044823 _ Rev. 31, 17 Nov. 2025.

(Verify that the scope complies with the latest revision of the applicable manual. To do so, check whether the revision indicated below matches the current revision of the manual available, as per the location specified on the Intranet:)

(According to Overhaul Manual_3044823 _ Rev. 31, 17 Nov. 2025.)


Nota: caso haja divergência, não seguir com as próximas etapas e notificar de forma imediata via e-mail a Engenharia para que seja realizada a atualização do escopo.

(Note: if there is any discrepancy, do not proceed with the following steps and immediately notify the responsible Engineering team via email so that the scope can be updated accordingly.)


	02
	PW100	REMOÇÃO / REMOVE	
Realizar a desmontagem da Front Cover e Rear Cover conforme Overhaul Manual 3044823, ATA 72-50-00, Seção “Disassembly”, Parágrafo 11., Etapa A., Figura 109 (High Pressure Turbine Disk Assembly): 
(Perform the disassembly of the Front Cover and Rear Cover in accordance with Overhaul Manual 3044823, ATA 72-50-00, Section “Disassembly”, Paragraph 11, Step A, Figure 109 (High Pressure Turbine Disk Assembly).)


	03
	PW100	REMOVER PALHETAS / REMOVE BLADES	
Realizar a remoção das HP Blades conforme Overhaul Manual 3044823, ATA 72-50-00, Seção “Disassembly”, Parágrafo 11., Etapa B., Figura 109 (Blade Removal): 
(Perform the removal of the HP Blades in accordance with Overhaul Manual 3044823, ATA 72-50-00, Section “Disassembly”, Paragraph 11, Step B, Figure 109 (Blade Removal)

	04
	PW100	INSPEÇÃO / INSPECTION	
Realizar a pesagem e identificação de cada HP Blades conforme Overhaul Manual 3044823, ATA 72-50-00, Seção “Subassembly-3”, Parágrafo 6., Etapa A., Figura 503 (Preparatory Steps): 
(Perform the post-NDT inspection of the part in accordance with CIR Manual 3043515, ATA 72-53-13, Section “Inspection/Check-01,” Paragraph 1, Step C, Figure 801 (Task 72-53-13-240-801). Assess acceptability limits per the referenced criteria.)
 

	05
	PW100	INSTALAR PALHETAS / INSTALL BLADES	
Realizar a instalação das HP Blades conforme Overhaul Manual 3044823, ATA 72-50-00, Seção “Subassembly-3”, Parágrafo 6., Etapa B., Figura 503 (Blade Installation): 
(Install the HP blades in accordance with Overhaul Manual 3044823, ATA 72-50-00, Section “Subassembly-3,” Paragraph 6, Step B, Figure 503 (Blade Installation).)

Qual foi o sentido de instalação das blades?
(What was the installation direction of the blades?)
 
 ( ) Sentido Horário 
(Clockwise direction.) 
 
( ) Sentido Anti-Horário 
(Counterclockwise Direction)


	06
	PW100	INSTALAR / INSTALL	
Realizar a instalação da Front Cover, Rear Cover e Interstage Air Seal conforme Overhaul Manual 3044823, ATA 72-50-00, Seção “Subassembly-3”, Parágrafo 6., Etapa D., Figura 503 (Front and Rear Cover Installation): 
(Perform the installation of the Front Cover, Rear Cover, and Interstage Air Seal in accordance with Overhaul Manual 3044823, ATA 72-50-00, Section “Subassembly-3”, Paragraph 6, Step D, Figure 503 (Front and Rear Cover Installation).)


	07
	PW100	REMOÇÃO / REMOVE	
Realizar a remoção dos trim na Front Cover e Interstage Air Seal conforme Overhaul Manual 3044823, ATA 72-50-00, Seção “Subassembly-3”, Parágrafo 7., Etapa E., Figura 510 (Trim Balancing of HP Rotor Assembly).
(Perform the removal of the trim on the Front Cover and Interstage Air Seal in accordance with Overhaul Manual 3044823, ATA 72-50-00, Section “Subassembly-3”, Paragraph 7, Step E, Figure 510 (Trim Balancing of HP Rotor Assembly).)


	08
	PW100	BALANCEAMENTO / BALANCING	
Realizar o balanceamento do conjunto de HP Disk conforme Overhaul Manual 3044823, ATA 72-50-00, Seção “Subassembly-3”, Parágrafo 6., Etapa E., Figura 505 (Detail Balancing of HP Turbine Disk Assembly (Method A)).
(Perform the balancing of the HP Disk assembly in accordance with Overhaul Manual 3044823, ATA 72-50-00, Section “Subassembly-3”, Paragraph 6, Step E, Figure 505 (Detail Balancing of HP Turbine Disk Assembly — Method A).)

(ref. Parágrafo E (11))
(ref. Paragraph E (11))

NCC:_______

Desbalanceamento inicial no Plano C: __________ [g.mm]
(Initial unbalance in Plane C:)

Ângulo do desbalanceamento inicial no Plano C: _______ [°]
(Initial unbalance angle in Plane C:)

Desbalanceamento inicial no Plano D: __________ [g.mm]
(Initial unbalance in Plane D:)

Ângulo do desbalanceamento inicial no Plano D: _______ [°]
(Initial unbalance angle in Plane D:)

(ref. Parágrafo E (13))
(ref. Paragraph E (13))

NCC:_______

Desbalanceamento final no Plano C: __________ [g.mm]
(Final unbalance in Plane C:) 

Ângulo do desbalanceamento final no Plano C: _______ [°]
(Final unbalance angle in Plane C:)

Desbalanceamento final no Plano D: __________ [g.mm]
(Final unbalance in Plane D:) 

Ângulo do desbalanceamento final no Plano D: _______ [°]
(Final unbalance angle in Plane D:)


	09
	PW100	INSTALAR / INSTALL	
Realizar a instalação dos trims no Front Cover e Interstage Air Seal conforme Overhaul Manual 3044823, ATA 72-50-00, Seção “Subassembly-3”, Parágrafo 7., Etapa E., Figura 510 (Trim Balancing of HP Rotor Assembly).
(Perform the installation of the trims on the Front Cover and Interstage Air Seal in accordance with Overhaul Manual 3044823, ATA 72-50-00, Section “Subassembly-3”, Paragraph 7, Step E, Figure 510 (Trim Balancing of HP Rotor Assembly).)


	10
	PW100	INSPEÇÃO / INSPECTION	Inspeção final. 
(Final Inspection.)

	OBSERVAÇÕES (Observation):
	ASSINATURA DO SOLICITANTE (Signature):
	DATA (Date):

	
	GUILHERME BRAGA
	12/05/2026


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department.)
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