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	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN: 01153

	             6858624
	                        KK25239
	050700
	

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	COMPRESSOR- ADOC 702131- EQUADOR
	       WHEEL 14º ST
	REVISÃO GERAL / OVERHAUL	1

	
	
	
	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	REMOVER TODOS PEDAÇOS DE PINOS.

REMOVE ALL PIECES OF PINS.

	2
	REPAIR SHOP	JATEAR / BLAST	ISOLAR E EXECUTAR SHOT PEEN NA FACE TRASEIRA, CONFORME AS INSTRUÇÕES DO WP 147 00, PÁGINAS 20 e 21 ANEXAS.                           VEJA A FIGURA ANEXA.

ISOLATE AND PERFORM SHOT PEEN ON THE REAR FACE, AS INSTRUCTED IN WP 147 00, PAGES 20 and 21 ANNEXED. SEE THE ATTACHED FIGURE.

	3
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO DIMENCIONAL DO DISH.

DIMENSIONAL DISH INSPECTION.

	4
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	5
	NDT	END- PARTICULAS MAGNETICAS / NOT - MAGNETIC PARTICLE	EXECUTAR MPI: ASTM E 1444.
APRESENTOU INDICAÇÃO? ( )SIM    ( )NÃO

RUN MPI: ASTM E 1444. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	6
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	7
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-D, LEVEL-4.
APRESENTOU INDICAÇÃO? ( )SIM     ( )NÃO
RUN FPI: ASTM E 1417, METHOD-D, LEVEL-4. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	8
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	9
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	INSTALAR AS PALHETAS E FRENA-LAS COM PINOS P/N= 6731108

INSTALL THE BLADES AND BRAKE THEM WITH P/N PINS = 6731108

	10
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
( )APROVADO       ( )REPROVADO

FINAL INSPECTION. ( )APPROVED ( )FAILED

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	


	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	
	Escolher um item.	Escolher um item.	

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 10/06/2026
(Date):

	[bookmark: Texto2]     
	VILSON BARBOSA
	10/06/2026


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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