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	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	AD0C702131
	        WHEEL 9º ST
	REVISÃO GERAL / OVERHAUL	1

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	REMOVER OS RESQUÍCIOS DE PINOS DOS FUROS DE FRENAGEM.

REMOVE ALL REMNANTS OF THE PINS FROM THE LOCKWIRE HOLES

	2
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.10

	3
	NDT	END- PARTICULAS MAGNETICAS / NOT - MAGNETIC PARTICLE	EXECUTAR MPI: ASTM E 1444.
APRESENTOU INDICAÇÃO?   (  ) SIM    (  ) NÃO
RUN MPI: ASTM E 1444. DID YOU PRESENT AN INDICATION? ( ) YES ( ) NO

	4
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10
CLEAR AS PER IP-0006, 3.10

	5
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-D, LEVEL 4.
APRESENTOU INDICAÇÕES?  (  )SIM         (  )NÃO

RUN FPI: ASTM E 1417, METHOD-D, LEVEL 4. DID YOU PRESENT INDICATIONS? ( )YES ( )NO

	6
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10
CLEAR AS PER IP-0006, 3.10

	7
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	MONTAR AS PALHETAS.
NOTA: Não frena-las.

ASSEMBLE THE BLADES. NOTE: Do not brake them.

	8
	REPAIR SHOP	BALANCEAMENTO / BALANCING	BALANCEAR O CONJUNTO.
BALANCE THE SET.

	9
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	FRENAR AS PALHETAS COM PINOS P/N= 6730907 E EXECUTAR STAK.
BRAKE THE VANES WITH PINS P/N= 6730907 AND PERFORM STAK.

	10
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
(  )APROVADO     (  )REPROVADO
FINAL INSPECTION. ( )APPROVED ( )FAILED

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 12/06/2026
(Date):

	[bookmark: Texto2]     
	AUGUSTO ROSA
	12/06/2026


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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