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	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:

	6894068
	61626
	054113
	02188

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	ADOT513855
	COMBUSTION LINER ASSY
	REVISÃO GERAL / OVERHAUL	01

	TSN:
	CSN:
	TSO:
	CSO:

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	TRATAMENTO TERMICO / HEAT TREATMENT	EXECUTAR TRATAMENTO TÉRMICO EM 1010°C, POR 30 MINUTOS COM AUSÊNCIA DE OXIGÊNIO.

PERFORM HEAT TREATMENT AT 1010°C FOR 30 MINUTES IN AN OXYGEN-FREE ATMOSPHERE

	2
	REPAIR SHOP	SOLDAR / WELDING	-SOLDAR TODAS AS TRINCAS EXTERNAS MARCADAS DE PINCEL. AMS-5798.
-SUAVISAR TODAS AS SOLDAS. TASK 72-47-00-300-801

PREPARE AND WELD ALL EXTERNAL CRACKS IDENTIFIED BY BRUSH MARKING, IN ACCORDANCE WITH AMS 5798.
BLEND/SMOOTH ALL WELDS TO ENSURE PROPER SURFACE FINISH.
PERFORM THE TASK IN ACCORDANCE WITH TASK 72-47-00-300-801


	3
	REPAIR SHOP	TRATAMENTO TERMICO / HEAT TREATMENT	EXECUTAR TRATAMENTO TÉRMICO EM 1010°C, POR 30 MINUTOS.

PERFORM HEAT TREATMENT AT 1010°C FOR 30 MINUTES.

	4
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.1

	5
	NDT	END- LIQUIDO PENETRANTE / NDT - FLUORESCENT PENETRANT INSPECTION	EXECUTAR FPI: ASTM E 1417, METHOD-A, LEVEL 3.
APRESENTOU INDICAÇÃO? (  )SIM          (  )NÃO

RUN FPI: ASTM E 1417, METHOD-A, LEVEL 3. DID YOU PRESENT AN INDICATION? ( )YES ( )NO

	6
	CHEMICAL CLEANING	LIMPAR / CLEAN	LIMPAR CONFORME A IP-0006, 3.10

CLEAR AS PER IP-0006, 3.1

	7
	T56A	INSPEÇÃO / INSPECTION	INSPEÇÃO FINAL.
(  )APROVADO                    (  )REPROVADO

FINAL INSPECTION. ( )APPROVED ( )FAILED

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
(Date):

	[bookmark: Texto2]     
	AUGUSTO ROSA
	30/06/2026


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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