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Descrição gerada automaticamente]
	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN:

	RR30000242
	VN1BLL0892
	053952
	TLN02015       

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	RRE-200270
	FUEL NOZZLE
	REVISÃO GERAL / OVERHAUL	1

	TSN:
	CSN:
	TSO:
	CSO:

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	
	Escolher um item.	ANALISE INICIAL DE DOCUMENTAÇÃO / INITIAL DOCUMENTATION ANALYSIS	REALIZAR ANÁLISE DOCUMENTAL - DIRETIVAS TÉCNICAS E TBO
(PERFORM DOCUMENTAL ANALYSIS - TECHNICAL DIRECTIVES AND TBO)

	
	ACESSÓRIOS	VERIFICAÇÃO DE RECEBIMENTO/ RECEIPT VERIFICATION	REALIZAR O RECEBIMENTO DO COMPONENTE REALIZANDO O REGISTRO DOS NÚMEROS
DE SÉRIE, PART NUMBER E CONDIÇÃO DE RECEBIMENTO DO ITEM
E SEUS COMPONENTES. REGISTRAR AS CONDIÇÕES ENCONTRADAS COM FOTOS E
ANOTAÇÕES EM RG-0007, CONFORME NECESSÁRIO.
(RECEIVE THE COMPONENT PERFORMING THE REGISTRATION OF THE SERIAL
NUMBER, PART NUMBER AND CONDITION OF RECEIPT OF THE ITEM AND ITS
COMPONENTS. RECORD CONDITIONS FOUND WITH PHOTOS AND NOTES IN RG-0007
AS NECESSARY.)

	
	ACESSÓRIOS	TESTE /TEST	SE POSSIVEL, REALIZAR TESTE INICIAL CONFORME CMM 73-16-01, REV. 2,
RR300 FUEL NOZZLE ASSEMBLY, TESTING.
(IF POSSIBLE, PERFORM INBOUND TEST ACCORDING TO CMM 73-16-01, REV. 2,
RR300 FUEL NOZZLE ASSEMBLY, TESTING)
Executado

	
	ACESSÓRIOS	DESMONTAGEM / DISASSEMBLY	REALIZAR DESMONTAGEM CONFORME CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, DISASSEMBLY
(PERFORM DISASSEMBLY ACCORDING TO CMM 73-16-01, REV. 2, RR300 FUEL
NOZZLE ASSEMBLY, DISASSEMBLY)

	
	ACESSÓRIOS	LIMPEZA - ACESSORIOS / CLEANING - ACCESSORIES	REALIZAR LIMPEZA CONFORME CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, CLEANING
(PERFORM CLEANING ACCORDING TO CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, CLEANING)

	
	ACESSÓRIOS	INSPEÇÃO / INSPECTION	REALIZAR INSPEÇÃO CONFORME CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, CHECK
(PERFORM CHECK ACCORDING TO CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, CHECK)

	
	ACESSÓRIOS	REPARAR - ACESSORIOS / REPAIR - ACCESSORIES	REALIZAR REPAROS NECESSÁRIOS CONFORME CMM 73-16-01, REV. 2, RR300 FUEL
NOZZLE ASSEMBLY, REPAIR
(PERFORM NECESSARY REPAIR ACCORDING TO CMM 73-16-01, REV. 2, RR300
FUEL NOZZLE ASSEMBLY, REPAIR)

	
	ACESSÓRIOS	MONTAG EM/ ASSEMBLY	REALIZAR MONTAGEM CONFORME CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, ASSEMBLY
(PERFORM ASSEMBLY ACCORDING TO CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, ASSEMBLY)

	
	ACESSÓRIOS	TESTE /TEST	REALIZAR TESTE CONFORME CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, TESTING
(PERFORM TEST ACCORDING TO CMM 73-16-01, REV. 2, RR300 FUEL NOZZLE
ASSEMBLY, TESTING)

	
	ACESSÓRIOS	APROVAÇÃO FINAL DO SERVLÇO REALIZADO / FINAL APPROVAL OF THE SERVICE	REALIZAR INSPEÇÃO FINAL CONFORME CMM 73-16-01, REV. 2, RR300 FUEL
NOZZLE ASSEMBLY
(PERFORM FINAL INSPECTION ACCORDING TO CMM 73-16-01, REV. 2, RR300
FUEL NOZZLE ASSEMBLY)

	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 
(Date):

	OVERHAUL
	BRUNO HENRIQUE ALVES
	06/07/2026


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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