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	REGISTRO
	REVISÃO
	04

	
	RECORD
	REVISION
	

	CODIGO | CODE
	SOLICITAÇÃO DE SERVIÇOS COMPLEMENTARES
	PÁGINA
	1/1

	IAS-RG-0103
	SUPPLEMENTARY REQUEST
	PAGE
	



	PN (PN):
	SN:
	Nº da OS (WO):
	TLN: 02623

	                    6873624
	MA20665
	054575
	

	Nº DO ARTIGO PRINCIPAL (Main Article):
	ARTIGO/PARTE (Article/Part):
	Serviço PrincipaL
(Main Service)
	QUANT:

	TU. 750283
	INLET VANE
	REVISÃO GERAL / OVERHAUL	1

	
	
	
	

	ITEM
(Item)
	[bookmark: _Hlk184222911]TAREFA
(Task)
	[bookmark: _Hlk184222919]ETAPA
(Step)
	DESCRIÇÃO
(Description)

	1
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	CORTAR 4- ALHETAS ASSINALADAS
E REMOVER O BRAZE DAS EXTREMIDADES.
VEJA AS INSTRUÇÕES NA PÁGINA 905 ANEXA.

CUT 4- MARKED FINS AND REMOVE THE BRAZE FROM THE EXTREMITIES. SEE INSTRUCTIONS ON PAGE 905 ATTACHED.

	2
	REPAIR SHOP	SOLDAR / WELDING	INSTALAR AS NOVAS ALHETAS 
E FECHAR PARTE DAS EXTREMIDADES, COM AMS 4774 ou AMS 5680.
VEJA A FIGURA ANEXA.

INSTALL THE NEW FINS AND CLOSE PART OF THE ENDS, WITH AMS 4774 or AMS 5680. SEE THE ATTACHED FIGURE.

	3
	REPAIR SHOP	REPAROS MANUAIS / MANUAL REPAIR	DESAMASSAR UM PONTO ASSINALADO
E POLIR COM LIXA FINA O BORDO DE ATAQUE E DE FUGA.

UNDENTING A MARKED POINT AND POLISH THE LEADING AND TRAILING EDGE WITH FINE SANDPAPER.

	4
	REPAIR SHOP	USINAGEM / MACHINING	USINAR O DIÂMETRO INTERNO, CONFORME MOSTRA O DESENHO ANEXO.
     CENTRAR PELO DIÂMETRO INTERNO DO FLANGE INTERNO E REMOVER APENAS AS PEQUENAS OVALIZAÇÕES.

MACHINE THE INNER DIAMETER, AS SHOWN IN THE ATTACHED DRAWING. CENTER BY THE INNER DIAMETER OF THE INNER FLANGE AND REMOVE ONLY THE SMALL OVALS

	5
	T56A	INSPEÇÃO / INSPECTION
	INSPEÇÃO FINAL.

FINAL INSPECTION.
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	OBSERVAÇÕES
(Observation):
	ASSINATURA DO SOLICITANTE 
(Signature):
	DATA 10/08/2026
(Date):

	[bookmark: Texto2]     
	VILSON BARBOSA
	10/08/2026


· Em caso de serviço externo, o fornecedor deverá ser indicado pelo setor de compras.
(In case of external service, the supplier must be indicated by the purchasing department)
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